Configure

1. Hostname (R1, R2, R3)

2. Interface fa, se(DCE, DTE)

3. Pc IP address

4. State Routing

R1->R2

R3

R2->R1

->R3

R3->R1

->R2

Ip route detsn\_NA destn\_Sm next\_hop\_address